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[bookmark: _Toc187374384]Introduction
This Architecture Conversion Report records the Florida District 4/6 Regional ITS Architecture (RITSA) update from its reference in the Architecture Reference for Cooperative and Intelligent Transportation (ARC-IT) Version 9.3 to ARC-IT Version 9.4. This report addresses notable results from the conversion process. 
ARC-IT is the national architecture reference for ITS. Version 9.4, per the https://www.arc-it.net/ website, includes new services for vehicle automation, maritime port information systems, and support for new vehicle-to-everything (V2X) communications methods; including networked V2X, wide area wireless (cellular), and introducing the use of multi-access edge computing (MEC).
[bookmark: _Toc187374385]Description of Changes
The architecture conversion process uses the Regional Architecture Development for Intelligent Transportation (RAD-IT) software Version 9.4 to convert the architecture to be compatible with ARC-IT Version 9.4. The process includes the following steps to accomplish the conversion.
· Architecture conversion: Conversion features in RAD-IT Version 9.4 convert the architecture database schema to be compatible with RAD-IT Version 9.4 and aligned to reference ARC-IT Version 9.4 content.
· Conversion analysis: Conversion information is produced by RAD-IT for the architecture conversion noting the changes made. The conversion information notes the schema and content changes, such as service splits or consolidations, element mapping changes, information flow changes, and communications standards changes. Analysis is required for each converted item to assess the appropriateness of each change for the architecture. 
· Architecture content update: The intent of the conversion process was to maintain the alignment of the converted Architecture content to the greatest extent possible with the pre-conversion Architecture content. Element physical object mapping changes, service package changes, information flow additions and adjustments, and the evolution of the standards mappings in ARC-IT Version 9.4 required changes to be made to the Architecture content. Unless it was necessary, no additional changes beyond those required to align the pre-conversion and converted architecture content were made. During the course of the Annual Architecture Maintenance Update, ARC-IT Version 9.4 features that could be considered as additional information to the Architecture will be assessed.
· Architecture website posting: The converted architecture will be posted to the Florida ITS Architecture website.
[bookmark: _Toc186514407][bookmark: _Toc187374386]Architecture Conversion Results 
The District 4/6 RITSA was converted to be compatible with ARC-IT Version 9.4. The following sections highlight the changes made to the architecture as a result of the conversion process.
[bookmark: _Toc186514408][bookmark: _Toc187374387]Architecture Inventory Elements
[bookmark: _Hlk186438406]For the conversion from 9.3 to 9.4 there were no changes to the architecture inventory of elements. 
[bookmark: _Toc187374388][bookmark: _Toc186514410]Architecture Information Flows
No architecture information flows were impacted by the conversion process. 
[bookmark: _Toc187374389]Architecture Functional Requirements 
Table 2 provides conversion results for architecture functional requirements impacted by the conversion process. The table shows the element impacted, the type of change made, the old functional object, number, and requirement, along with the new functional object, number, and requirement to display the change made.
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[bookmark: _Toc237872392]Table 1. Conversion Analysis of Functional Requirements
	Element Name
	Change
	Old Functional Object
	Old Num
	Old Req
	New Functional Object
	New Num
	New Req

	BCT Fixed Route Vehicles
	Modified
	Vehicle Control Automation
	3
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and a stationary object, based on the proximity of other objects to the vehicle and the current speed and direction of the vehicle.
	Vehicle Control Automation
	3
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and another objects, based on the proximity and vectors of other objects relative to the vehicle and the current speed and direction of the vehicle.

	BCT Fixed Route Vehicles
	Modified
	Vehicle Control Warning
	2
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and a stationary object to warn the driver, based on the proximity of other objects to the vehicle, roadway characteristics, and the current speed and direction of the vehicle.
	Vehicle Control Warning
	2
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and another object to warn the driver, based on the proximity and vectors of other objects to the vehicle, roadway characteristics, and the current speed and direction of the vehicle.

	Broward County CAV Field Equipment
	Modified
	RSE Map Management
	10
	The field element shall provide intersection geometry updates to proximate Vehicles.
	RSE Map Management
	10
	The field element shall acquire intersection geometry information from mapping centers.

	Broward County CAV Field Equipment
	Modified
	RSE Map Management
	12
	The field element shall provide roadway geometry updates to proximate Vehicles.
	RSE Map Management
	12
	The field element shall acquire roadway geometry information from mapping centers.

	Broward County CAV Field Equipment
	Modified
	RSE Map Management
	9
	The field element shall provide basemap updates to proximate Vehicles.
	RSE Map Management
	9
	The field element shall acquire basemap updates from mapping centers.

	Broward County Field Equipment
	Replaced
	Roadway Basic Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.
	Roadway Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.

	Broward County Field Equipment
	Replaced
	Roadway Basic Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.
	Roadway Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.

	Broward County Field Equipment
	Replaced
	Roadway Basic Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.
	Roadway Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.

	Broward County Field Equipment
	Replaced
	Roadway Basic Surveillance
	6
	The field element shall collect, process, and send traffic images to the center for further wrong way vehicle entries analysis and detection.
	Roadway Surveillance
	6
	The field element shall collect, process, and send traffic images to the center for further wrong way vehicle entries analysis and detection.

	City of Boca Raton Traffic Control Equipment
	Replaced
	Roadway Basic Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.
	Roadway Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.

	City of Boca Raton Traffic Control Equipment
	Replaced
	Roadway Basic Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.
	Roadway Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.

	City of Boca Raton Traffic Control Equipment
	Replaced
	Roadway Basic Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.
	Roadway Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.

	City of Boca Raton Traffic Control Equipment
	Replaced
	Roadway Basic Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.
	Roadway Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.

	City of Fort Pierce Field Equipment
	Replaced
	Roadway Basic Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.
	Roadway Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.

	City of Fort Pierce Field Equipment
	Replaced
	Roadway Basic Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.
	Roadway Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.

	City of Fort Pierce Field Equipment
	Replaced
	Roadway Basic Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.
	Roadway Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.

	City of Fort Pierce Field Equipment
	Replaced
	Roadway Basic Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.
	Roadway Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.

	City of Port St. Lucie Field Equipment
	Replaced
	Roadway Basic Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.
	Roadway Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.

	City of Port St. Lucie Field Equipment
	Replaced
	Roadway Basic Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.
	Roadway Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.

	City of Port St. Lucie Field Equipment
	Replaced
	Roadway Basic Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.
	Roadway Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.

	City of Port St. Lucie Field Equipment
	Replaced
	Roadway Basic Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.
	Roadway Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.

	Commercial Vehicle
	Modified
	Vehicle Control Warning
	2
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and a stationary object to warn the driver, based on the proximity of other objects to the vehicle, roadway characteristics, and the current speed and direction of the vehicle.
	Vehicle Control Warning
	2
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and another object to warn the driver, based on the proximity and vectors of other objects to the vehicle, roadway characteristics, and the current speed and direction of the vehicle.

	Commercial Vehicle
	Replaced
	Vehicle Intersection Warning
	1
	Vehicle shall provide vehicle path information to identify if vehicle is performing an unpermitted movement at an intersection such as a stop sign violation or running a red light.
	Vehicle Intersection Movement
	1
	The vehicle shall provide vehicle path information to identify if vehicle is performing an unpermitted movement at an intersection such as a stop sign violation or running a red light.

	Commercial Vehicle
	Replaced
	Vehicle Intersection Warning
	2
	Vehicle shall provide data describing the vehicle's location in three dimensions, heading, speed, acceleration, braking status, and size.
	Vehicle Intersection Movement
	2
	The vehicle shall provide data describing the vehicle's location in three dimensions, heading, speed, acceleration, braking status, and size.

	Commercial Vehicle
	Replaced
	Vehicle Intersection Warning
	3
	The vehicle shall receive intersection signal timing information in order for the vehicle to determine if it will safely cross the intersection given its current location and speed.
	Vehicle Intersection Movement
	3
	The vehicle shall receive intersection signal timing information in order for the vehicle to determine if it will safely cross the intersection given its current location and speed.

	Commercial Vehicle
	Replaced
	Vehicle Intersection Warning
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.
	Vehicle Intersection Movement
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.

	Commercial Vehicle
	Replaced
	Vehicle Intersection Warning
	5
	The vehicle shall receive warning from the infrastructure if an intersection violation appears to be imminent.
	Vehicle Intersection Movement
	5
	The vehicle shall receive warning from the infrastructure if an intersection violation appears to be imminent.

	Commercial Vehicle
	Replaced
	Vehicle Intersection Warning
	6
	The vehicle shall provide to the driver a warning if it looks like the vehicle will go through the intersection after the signal has turned red.
	Vehicle Intersection Movement
	6
	The vehicle shall provide to the driver a warning if it looks like the vehicle will go through the intersection after the signal has turned red.

	County and Local CAV Field Equipment
	Modified
	RSE Map Management
	10
	The field element shall provide intersection geometry updates to proximate Vehicles.
	RSE Map Management
	10
	The field element shall acquire intersection geometry information from mapping centers.

	County and Local CAV Field Equipment
	Modified
	RSE Map Management
	9
	The field element shall provide basemap updates to proximate Vehicles.
	RSE Map Management
	9
	The field element shall acquire basemap updates from mapping centers.

	County Fire EMS/Rescue Vehicles
	Replaced
	Vehicle Intersection Warning
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.
	Vehicle Intersection Movement
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.

	County Sheriffs Vehicles
	Replaced
	Vehicle Intersection Warning
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.
	Vehicle Intersection Movement
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.

	FDOT District 4 CAV Field Equipment
	Modified
	RSE Intersection Management
	4
	The field element shall receive signal priority requests from commercial vehicles and forward to the traffic signal controller.
	RSE Intersection Management
	4
	The field element shall receive signal priority/preemption requests from  vehicles.

	FDOT District 4 Field Equipment
	Replaced
	Roadway Basic Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.
	Roadway Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.

	FDOT District 4 Field Equipment
	Replaced
	Roadway Basic Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.
	Roadway Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.

	FDOT District 4 Field Equipment
	Replaced
	Roadway Basic Surveillance
	3
	The field element shall collect, digitize, and send multimodal crossing and high occupancy vehicle (HOV), and high occupancy toll (HOT) lane sensor data to the center for further analysis and storage.
	Roadway Surveillance
	3
	The field element shall collect, digitize, and send multimodal crossing and high occupancy vehicle (HOV), and high occupancy toll (HOT) lane sensor data to the center for further analysis and storage.

	FDOT District 4 Field Equipment
	Replaced
	Roadway Basic Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.
	Roadway Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.

	FDOT District 6 95 Express Ramp Warning Gates
	Modified
	RSE Road Closure Management
	1
	The field element shall communicate with qualified connected vehicles and barrier control systems to support local road closure management.
	RSE Road Closure Management
	1
		The field element shall communicate with qualified connected vehicles and barrier control systems to support local road closure management.

	FDOT District 6 CAV Field Equipment
	Modified
	RSE Intersection Management
	4
	The field element shall receive signal priority requests from commercial vehicles and forward to the traffic signal controller.
	RSE Intersection Management
	4
	The field element shall receive signal priority/preemption requests from  vehicles.

	FDOT District 6 CAV Field Equipment
	Modified
	RSE Map Management
	10
	The field element shall provide intersection geometry updates to proximate Vehicles.
	RSE Map Management
	10
	The field element shall acquire intersection geometry information from mapping centers.

	FDOT District 6 CAV Field Equipment
	Modified
	RSE Map Management
	11
	The field element shall provide parking facility geometry information to proximate Personal devices.
	RSE Map Management
	11
	The field element shall acquire parking facility geometry information from mapping centers.

	FDOT District 6 CAV Field Equipment
	Modified
	RSE Map Management
	12
	The field element shall provide roadway geometry updates to proximate Vehicles.
	RSE Map Management
	12
	The field element shall acquire roadway geometry information from mapping centers.

	FDOT District 6 CAV Field Equipment
	Modified
	RSE Map Management
	9
	The field element shall provide basemap updates to proximate Vehicles.
	RSE Map Management
	9
	The field element shall acquire basemap updates from mapping centers.

	FDOT District 6 CAV Field Equipment
	Modified
	RSE Traveler Information Communications
	13
	The field element shall provide data about transit vehicle movement to approaching vehicles
	RSE Traveler Information Communications
	13
	The field element shall provide data about transit vehicle movement to approaching vehicles.

	FDOT District 6 Signal Field Equipment
	Replaced
	Roadway Basic Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.
	Roadway Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.

	FDOT District 6 Signal Field Equipment
	Replaced
	Roadway Basic Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.
	Roadway Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.

	FDOT District 6 Signal Field Equipment
	Replaced
	Roadway Basic Surveillance
	3
	The field element shall collect, digitize, and send multimodal crossing and high occupancy vehicle (HOV), and high occupancy toll (HOT) lane sensor data to the center for further analysis and storage.
	Roadway Surveillance
	3
	The field element shall collect, digitize, and send multimodal crossing and high occupancy vehicle (HOV), and high occupancy toll (HOT) lane sensor data to the center for further analysis and storage.

	FDOT District 6 Signal Field Equipment
	Replaced
	Roadway Basic Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.
	Roadway Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.

	FDOT District 6 Signal Field Equipment
	Replaced
	Roadway Basic Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.
	Roadway Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.

	FDOT District 6 Signal Field Equipment
	Replaced
	Roadway Basic Surveillance
	6
	The field element shall collect, process, and send traffic images to the center for further wrong way vehicle entries analysis and detection.
	Roadway Surveillance
	6
	The field element shall collect, process, and send traffic images to the center for further wrong way vehicle entries analysis and detection.

	FDOT District 6 SunGuide Field Equipment
	Replaced
	Roadway Basic Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.
	Roadway Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.

	FDOT District 6 SunGuide Field Equipment
	Replaced
	Roadway Basic Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.
	Roadway Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.

	FDOT District 6 SunGuide Field Equipment
	Replaced
	Roadway Basic Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.
	Roadway Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.

	FDOT District 6 SunGuide Field Equipment
	Replaced
	Roadway Basic Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.
	Roadway Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.

	Florida Highway Patrol Vehicles
	Modified
	Vehicle Control Warning
	2
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and a stationary object to warn the driver, based on the proximity of other objects to the vehicle, roadway characteristics, and the current speed and direction of the vehicle.
	Vehicle Control Warning
	2
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and another object to warn the driver, based on the proximity and vectors of other objects to the vehicle, roadway characteristics, and the current speed and direction of the vehicle.

	Florida Highway Patrol Vehicles
	Replaced
	Vehicle Intersection Warning
	1
	Vehicle shall provide vehicle path information to identify if vehicle is performing an unpermitted movement at an intersection such as a stop sign violation or running a red light.
	Vehicle Intersection Movement
	1
	The vehicle shall provide vehicle path information to identify if vehicle is performing an unpermitted movement at an intersection such as a stop sign violation or running a red light.

	Florida Highway Patrol Vehicles
	Replaced
	Vehicle Intersection Warning
	2
	Vehicle shall provide data describing the vehicle's location in three dimensions, heading, speed, acceleration, braking status, and size.
	Vehicle Intersection Movement
	2
	The vehicle shall provide data describing the vehicle's location in three dimensions, heading, speed, acceleration, braking status, and size.

	Florida Highway Patrol Vehicles
	Replaced
	Vehicle Intersection Warning
	3
	The vehicle shall receive intersection signal timing information in order for the vehicle to determine if it will safely cross the intersection given its current location and speed.
	Vehicle Intersection Movement
	3
	The vehicle shall receive intersection signal timing information in order for the vehicle to determine if it will safely cross the intersection given its current location and speed.

	Florida Highway Patrol Vehicles
	Replaced
	Vehicle Intersection Warning
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.
	Vehicle Intersection Movement
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.

	Florida Highway Patrol Vehicles
	Replaced
	Vehicle Intersection Warning
	5
	The vehicle shall receive warning from the infrastructure if an intersection violation appears to be imminent.
	Vehicle Intersection Movement
	5
	The vehicle shall receive warning from the infrastructure if an intersection violation appears to be imminent.

	Florida Highway Patrol Vehicles
	Replaced
	Vehicle Intersection Warning
	6
	The vehicle shall provide to the driver a warning if it looks like the vehicle will go through the intersection after the signal has turned red.
	Vehicle Intersection Movement
	6
	The vehicle shall provide to the driver a warning if it looks like the vehicle will go through the intersection after the signal has turned red.

	Indian River County Field Equipment
	Replaced
	Roadway Basic Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.
	Roadway Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.

	Indian River County Field Equipment
	Replaced
	Roadway Basic Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.
	Roadway Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.

	Indian River County Field Equipment
	Replaced
	Roadway Basic Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.
	Roadway Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.

	Indian River County Field Equipment
	Replaced
	Roadway Basic Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.
	Roadway Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.

	Local Fire/EMS Vehicles
	Modified
	Vehicle Control Warning
	2
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and a stationary object to warn the driver, based on the proximity of other objects to the vehicle, roadway characteristics, and the current speed and direction of the vehicle.
	Vehicle Control Warning
	2
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and another object to warn the driver, based on the proximity and vectors of other objects to the vehicle, roadway characteristics, and the current speed and direction of the vehicle.

	Local Fire/EMS Vehicles
	Replaced
	Vehicle Intersection Warning
	1
	Vehicle shall provide vehicle path information to identify if vehicle is performing an unpermitted movement at an intersection such as a stop sign violation or running a red light.
	Vehicle Intersection Movement
	1
	The vehicle shall provide vehicle path information to identify if vehicle is performing an unpermitted movement at an intersection such as a stop sign violation or running a red light.

	Local Fire/EMS Vehicles
	Replaced
	Vehicle Intersection Warning
	2
	Vehicle shall provide data describing the vehicle's location in three dimensions, heading, speed, acceleration, braking status, and size.
	Vehicle Intersection Movement
	2
	The vehicle shall provide data describing the vehicle's location in three dimensions, heading, speed, acceleration, braking status, and size.

	Local Fire/EMS Vehicles
	Replaced
	Vehicle Intersection Warning
	3
	The vehicle shall receive intersection signal timing information in order for the vehicle to determine if it will safely cross the intersection given its current location and speed.
	Vehicle Intersection Movement
	3
	The vehicle shall receive intersection signal timing information in order for the vehicle to determine if it will safely cross the intersection given its current location and speed.

	Local Fire/EMS Vehicles
	Replaced
	Vehicle Intersection Warning
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.
	Vehicle Intersection Movement
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.

	Local Fire/EMS Vehicles
	Replaced
	Vehicle Intersection Warning
	5
	The vehicle shall receive warning from the infrastructure if an intersection violation appears to be imminent.
	Vehicle Intersection Movement
	5
	The vehicle shall receive warning from the infrastructure if an intersection violation appears to be imminent.

	Local Fire/EMS Vehicles
	Replaced
	Vehicle Intersection Warning
	6
	The vehicle shall provide to the driver a warning if it looks like the vehicle will go through the intersection after the signal has turned red.
	Vehicle Intersection Movement
	6
	The vehicle shall provide to the driver a warning if it looks like the vehicle will go through the intersection after the signal has turned red.

	Local Police Vehicles
	Modified
	Vehicle Control Warning
	2
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and a stationary object to warn the driver, based on the proximity of other objects to the vehicle, roadway characteristics, and the current speed and direction of the vehicle.
	Vehicle Control Warning
	2
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and another object to warn the driver, based on the proximity and vectors of other objects to the vehicle, roadway characteristics, and the current speed and direction of the vehicle.

	Local Police Vehicles
	Replaced
	Vehicle Intersection Warning
	1
	Vehicle shall provide vehicle path information to identify if vehicle is performing an unpermitted movement at an intersection such as a stop sign violation or running a red light.
	Vehicle Intersection Movement
	1
	The vehicle shall provide vehicle path information to identify if vehicle is performing an unpermitted movement at an intersection such as a stop sign violation or running a red light.

	Local Police Vehicles
	Replaced
	Vehicle Intersection Warning
	2
	Vehicle shall provide data describing the vehicle's location in three dimensions, heading, speed, acceleration, braking status, and size.
	Vehicle Intersection Movement
	2
	The vehicle shall provide data describing the vehicle's location in three dimensions, heading, speed, acceleration, braking status, and size.

	Local Police Vehicles
	Replaced
	Vehicle Intersection Warning
	3
	The vehicle shall receive intersection signal timing information in order for the vehicle to determine if it will safely cross the intersection given its current location and speed.
	Vehicle Intersection Movement
	3
	The vehicle shall receive intersection signal timing information in order for the vehicle to determine if it will safely cross the intersection given its current location and speed.

	Local Police Vehicles
	Replaced
	Vehicle Intersection Warning
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.
	Vehicle Intersection Movement
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.

	Local Police Vehicles
	Replaced
	Vehicle Intersection Warning
	5
	The vehicle shall receive warning from the infrastructure if an intersection violation appears to be imminent.
	Vehicle Intersection Movement
	5
	The vehicle shall receive warning from the infrastructure if an intersection violation appears to be imminent.

	Local Police Vehicles
	Replaced
	Vehicle Intersection Warning
	6
	The vehicle shall provide to the driver a warning if it looks like the vehicle will go through the intersection after the signal has turned red.
	Vehicle Intersection Movement
	6
	The vehicle shall provide to the driver a warning if it looks like the vehicle will go through the intersection after the signal has turned red.

	Local Transit Operators Vehicles
	Replaced
	Vehicle Intersection Warning
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.
	Vehicle Intersection Movement
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.

	Miami-Dade CAV Field Equipment
	Modified
	RSE Map Management
	10
	The field element shall provide intersection geometry updates to proximate Vehicles.
	RSE Map Management
	10
	The field element shall acquire intersection geometry information from mapping centers.

	Miami-Dade CAV Field Equipment
	Modified
	RSE Map Management
	9
	The field element shall provide basemap updates to proximate Vehicles.
	RSE Map Management
	9
	The field element shall acquire basemap updates from mapping centers.

	Miami-Dade Traffic Control Equipment
	Modified
	RSE Road Closure Management
	1
	The field element shall communicate with qualified connected vehicles and barrier control systems to support local road closure management.
	RSE Road Closure Management
	1
		The field element shall communicate with qualified connected vehicles and barrier control systems to support local road closure management.

	Miami-Dade Traffic Control Equipment
	Replaced
	Roadway Basic Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.
	Roadway Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.

	Miami-Dade Traffic Control Equipment
	Replaced
	Roadway Basic Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.
	Roadway Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.

	Miami-Dade Traffic Control Equipment
	Replaced
	Roadway Basic Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.
	Roadway Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.

	Miami-Dade Traffic Control Equipment
	Replaced
	Roadway Basic Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.
	Roadway Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.

	Miami-Dade Transit Metrobuses
	Modified
	Vehicle Control Warning
	2
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and a stationary object to warn the driver, based on the proximity of other objects to the vehicle, roadway characteristics, and the current speed and direction of the vehicle.
	Vehicle Control Warning
	2
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and another object to warn the driver, based on the proximity and vectors of other objects to the vehicle, roadway characteristics, and the current speed and direction of the vehicle.

	Miami-Dade Transit Metrobuses
	Replaced
	Vehicle Intersection Warning
	1
	Vehicle shall provide vehicle path information to identify if vehicle is performing an unpermitted movement at an intersection such as a stop sign violation or running a red light.
	Vehicle Intersection Movement
	1
	The vehicle shall provide vehicle path information to identify if vehicle is performing an unpermitted movement at an intersection such as a stop sign violation or running a red light.

	Miami-Dade Transit Metrobuses
	Replaced
	Vehicle Intersection Warning
	2
	Vehicle shall provide data describing the vehicle's location in three dimensions, heading, speed, acceleration, braking status, and size.
	Vehicle Intersection Movement
	2
	The vehicle shall provide data describing the vehicle's location in three dimensions, heading, speed, acceleration, braking status, and size.

	Miami-Dade Transit Metrobuses
	Replaced
	Vehicle Intersection Warning
	3
	The vehicle shall receive intersection signal timing information in order for the vehicle to determine if it will safely cross the intersection given its current location and speed.
	Vehicle Intersection Movement
	3
	The vehicle shall receive intersection signal timing information in order for the vehicle to determine if it will safely cross the intersection given its current location and speed.

	Miami-Dade Transit Metrobuses
	Replaced
	Vehicle Intersection Warning
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.
	Vehicle Intersection Movement
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.

	Miami-Dade Transit Metrobuses
	Replaced
	Vehicle Intersection Warning
	5
	The vehicle shall receive warning from the infrastructure if an intersection violation appears to be imminent.
	Vehicle Intersection Movement
	5
	The vehicle shall receive warning from the infrastructure if an intersection violation appears to be imminent.

	Miami-Dade Transit Metrobuses
	Replaced
	Vehicle Intersection Warning
	6
	The vehicle shall provide to the driver a warning if it looks like the vehicle will go through the intersection after the signal has turned red.
	Vehicle Intersection Movement
	6
	The vehicle shall provide to the driver a warning if it looks like the vehicle will go through the intersection after the signal has turned red.

	Palm Beach County Field Equipment
	Replaced
	Roadway Basic Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.
	Roadway Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.

	Palm Beach County Field Equipment
	Replaced
	Roadway Basic Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.
	Roadway Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.

	Palm Beach County Field Equipment
	Replaced
	Roadway Basic Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.
	Roadway Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.

	Palm Beach County Field Equipment
	Replaced
	Roadway Basic Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.
	Roadway Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.

	St. Lucie County Field Equipment
	Replaced
	Roadway Basic Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.
	Roadway Surveillance
	1
	The field element shall collect, process, digitize, and send traffic sensor data (speed, volume, and occupancy) to the center for further analysis and storage, under center control.

	St. Lucie County Field Equipment
	Replaced
	Roadway Basic Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.
	Roadway Surveillance
	2
	The field element shall collect, process, and send traffic images to the center for further analysis and distribution.

	St. Lucie County Field Equipment
	Replaced
	Roadway Basic Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.
	Roadway Surveillance
	4
	The field element shall return sensor and CCTV system operational status to the controlling center.

	St. Lucie County Field Equipment
	Replaced
	Roadway Basic Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.
	Roadway Surveillance
	5
	The field element shall return sensor and CCTV system fault data to the controlling center for repair.

	Vehicles
	Modified
	Vehicle Control Automation
	3
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and a stationary object, based on the proximity of other objects to the vehicle and the current speed and direction of the vehicle.
	Vehicle Control Automation
	3
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and another objects, based on the proximity and vectors of other objects relative to the vehicle and the current speed and direction of the vehicle.

	Vehicles
	Modified
	Vehicle Control Warning
	2
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and a stationary object to warn the driver, based on the proximity of other objects to the vehicle, roadway characteristics, and the current speed and direction of the vehicle.
	Vehicle Control Warning
	2
	The vehicle shall evaluate the likelihood of a collision between two vehicles or a vehicle and another object to warn the driver, based on the proximity and vectors of other objects to the vehicle, roadway characteristics, and the current speed and direction of the vehicle.

	Vehicles
	Replaced
	Vehicle Intersection Warning
	1
	Vehicle shall provide vehicle path information to identify if vehicle is performing an unpermitted movement at an intersection such as a stop sign violation or running a red light.
	Vehicle Intersection Movement
	1
	The vehicle shall provide vehicle path information to identify if vehicle is performing an unpermitted movement at an intersection such as a stop sign violation or running a red light.

	Vehicles
	Replaced
	Vehicle Intersection Warning
	2
	Vehicle shall provide data describing the vehicle's location in three dimensions, heading, speed, acceleration, braking status, and size.
	Vehicle Intersection Movement
	2
	The vehicle shall provide data describing the vehicle's location in three dimensions, heading, speed, acceleration, braking status, and size.

	Vehicles
	Replaced
	Vehicle Intersection Warning
	3
	The vehicle shall receive intersection signal timing information in order for the vehicle to determine if it will safely cross the intersection given its current location and speed.
	Vehicle Intersection Movement
	3
	The vehicle shall receive intersection signal timing information in order for the vehicle to determine if it will safely cross the intersection given its current location and speed.

	Vehicles
	Replaced
	Vehicle Intersection Warning
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.
	Vehicle Intersection Movement
	4
	The vehicle shall be capable of providing warnings to the driver based upon information received regarding pedestrians, cyclists, and other non-motorized users that are sharing the roadway with the vehicle.

	Vehicles
	Replaced
	Vehicle Intersection Warning
	5
	The vehicle shall receive warning from the infrastructure if an intersection violation appears to be imminent.
	Vehicle Intersection Movement
	5
	The vehicle shall receive warning from the infrastructure if an intersection violation appears to be imminent.

	Vehicles
	Replaced
	Vehicle Intersection Warning
	6
	The vehicle shall provide to the driver a warning if it looks like the vehicle will go through the intersection after the signal has turned red.
	Vehicle Intersection Movement
	6
	The vehicle shall provide to the driver a warning if it looks like the vehicle will go through the intersection after the signal has turned red.
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